CHAMBER TRIGGER LINKS: system interconnections CTL1v11: Padova, 28 oct 1998

C4

C3

C2

C1

SB SB

SB

SB

SB

CTL1(*1)

CTL2(*2)

CTL3(*3)

CTL4(*4)

(*1) Station 1 Trigger Link Φ 1(0:11) Radial of first track Φ b1(0:9) Bending of first track Q1(0:2) Quality of first track Φ 2(0:11) same for second track Φ b2(0:9) Q2(0:2)

QΘ Quality of theta SL trigger

(*2) Station 2 Trigger Link Φ 1(0:11) Radial of first track Φ b1(0:9) Bending of first track Q1(0:2) Quality of first track Φ 2(0:11) same for second track Φ b2(0:9) Q2(0:2)

QΘ Quality of theta SL trigger

(*3) Station 3 Trigger Link Φ 1(0:11) Radial of first track Q1(0:1) Quality of first track Φ 2(0:11) same for second track Q2(0:1)

QΘ Quality of theta SL trigger

(*4) Station 4 Trigger Link Φ 1(0:11) Radial of first track Q1(0:1) Quality of first track Φ 2(0:11) same for second track Q2(0:1)

3x20 wires twisted flat cable 3x20 wires twisted flat cable 2x20 wires twisted flat cable 20 wires twisted flat cable

STL(*5)

(*5) Sector Trigger Link

2x12 fibers ribbon cable

SB: Server Board SU: Sorting Unit TTX: Trigger Transmitter

Chamber Trigger Links

Sector Trigger Link SU TTX

Θ(0:31) Theta SL hits Θ(0:31) Theta SL hits

Θ(0:15) Theta SL hits

To Regional Trigger